## Out with the Old... Install with the new!

The NEW fitting of choice for professional plumbers throughout the UK.

GET YOUR FREE SAMPLE PACK Find your nearest stockist

## Love at first sight

With a huge range of accreditations for complete reassurance

GET YOUR FREE SAMPLE PACK Find your nearest stockist

## Fit with confidence

With our new In-Cert® Pipe Stiffener giving real confidence of joint integrity

GET YOUR FREE SAMPLE PACK Find your nearest stockist

## THE ONLY SYSTEM YOU NEED

Say goodbye to your old push fit plumbing system with the introduction of PolyPlumb® Enhanced. The NEW fitting of choice for professional plumbers throughout the UK.

So you now have a complete system in grey and white for all of your plumbing and heating jobs, whether it’s first fix or a new renovation project, PolyPlumb® Enhanced is the only system you need.

But don’t just take our word for it. Click on the button below to grab your FREE PolyPlumb® Enhanced sample today.

GET YOUR FREE SAMPLE PACK

## POLYPLUMB® ENHANCED : THE FUTURE OF PUSH FIT-PLUMBING

### Revolutionise your 1st and 2nd fix installations with PolyPlumb® Enhanced.

Building on over 25 years of trust, we’ve listened to UK contractors like you and created the ultimate push-fit plumbing system. PolyPlumb Enhanced delivers superior performance and addresses the challenges you face daily.

Experience the difference first-hand.

GET YOUR FREE SAMPLE PACK

Secure Push-Fit Jointing When combined with the In-Cert® Pipe Stiffener, the unique fitting body centralises the pipe and with a twist provides feedback giving confidence that the joint has been made.

NEW In-Cert® Pipe Stiffener In-Cert® Pipe Stiffener featuring patented feedback technology.

New Design Cap Nut Improved design giving the fitting a fresh new look

O-Ring Featuring our trusted pre-lubricated EPDM O-Ring, ensuring continued joint integrity

Stainless Steel Grab Ring Proven high-performance stainless-steel grab ring for superb joint integrity.

## Stainless Steel Grab Ring.

### High-Performance Stainless-Steel Grab Ring

For 25 years PolyPlumb® has been the grey fitting of choice for professional installers. Now Enhanced and available in white for the first time, PolyPlumb® Enhanced is the only system you will ever need.

Secure Push-Fit Jointing When combined with the In-Cert® Pipe Stiffener, the unique fitting body centralises the pipe and with a twist provides feedback giving confidence that the joint has been made.

NEW In-Cert® Pipe Stiffener In-Cert® Pipe Stiffener featuring patented feedback technology.

New Design Nap Cut Improve design giving the fitting a fresh new look

O-Ring Featuring our trusted pre-lubricated EPDM O-Ring, ensuring continued joint integrity

Stainless Steel Grab Ring Proven high performance stainless-steel grab ring for superb joint integrity.

### Experience the difference first-hand.

GET YOUR FREE SAMPLE PACK

## Giving Installers and Contractors a Voice

Our Popular PolyPlumb® range has been enhanced with a fresh new look and a host of features. Best of all, it's now available in both grey and white, giving you a complete solution for any plumbing and heating job.

Request your sample pack today and experience PolyPlumb® Enhanced. We're confident it will be love at first SITE.

Experience the difference first-hand.

GET YOUR FREE SAMPLE PACK

## POLYPLUMB® ENHANCED IN A STOCKIST NEAR YOU NOW.

Search for your nearest PolyPlumb® Enhanced stockist by simply entering your postcode below:

## FAQs

We understand that you may have questions about our new PolyPlumb® Enhanced system that’s why we’ve pulled together a list of the most frequently asked questions.

Other than the colour, none! The grey and white PolyPlumb® Enhanced fittings are manufactured to the same standard (BS 7291 Parts 1, 2 & 3), offer the same 50-year guarantee, and are manufactured to the same tolerances and dimensions.

PolyPlumb® Enhanced fittings are compatible with copper pipe. When using copper pipe with these fittings, ensure a clean cut by using a rotor or wheel cutter. Deburr the cut end before inserting the pipe into the fitting. Please note: PolyPlumb® Enhanced In-Cert® technology is not compatible with copper pipe installations i.e. you will not feel the haptic click if you twist the pipe within the fitting.

While PolyPlumb® Enhanced fittings are generally reusable, there’s one important exception: the stainless-steel grab ring.

When reinstalling the fitting, always use a new grab ring.

To demount PolyPlumb® Enhanced fittings:

i. Remove the cap nut.

ii. Carefully pull the pipe out.

iii. Cut off the grab ring with side cutters.

iv. Peel the grab ring from the pipe.

v. Insert a new grab ring into the fitting.

vi. Reassemble as needed

Important: If the pipe has any scores or scratches, cut it back to a clean section before reinstallation.

Installing PolyPlumb® Enhanced fittings is as easy as installing the original PolyPlumb® fittings. Follow these simple steps:

i. Locate the ‘K’ mark on the pipe and cut it precisely at that point.
ii. Carefully examine the cut end of the pipe for any scratches or imperfections.
iii. Place the In-Cert® pipe stiffener into the cut end of the pipe.
iv. Gently push the pipe into the fitting until it reaches the next ‘K’ mark. v. Give the pipe a slight push and twist to ensure a secure fit. If using an In-Cert pipe stiffener, you will feel the ‘haptic click’ if you have made the joint successfully.

That’s it! Your PolyPlumb® Enhanced fitting is now securely installed.

Plastic pipes, like copper pipes, can freeze. While they are more resistant to freezing than copper, they can still be affected. Frozen water expands, potentially causing plastic pipes to stretch. To prevent this and ensure a reliable water supply, it’s crucial to insulate plastic pipes and fittings in the same ways you would copper.

No. PolyPlumb® Enhanced fittings come pre-lubricated straight from the factory. If you disassemble the joint and think the ‘O’ ring is dry, you can re-lubricate it with a WRAS approved aerosol lubricant.

PolyPlumb® Enhanced fittings and Pro-Straight® pipe, made with polybutylene, are perfect for both hard and soft water regions. Polybutylene’s inertness to chemical reactions means it resists scale buildup and corrosion, ensuring a long-lasting and efficient plumbing system. Unlike other materials, PolyPlumb® Enhanced is unaffected by water quality, making it a reliable choice for any environment.

Yes, polybutylene pipe can be used with compression fittings. However, it’s essential to follow a few guidelines for a secure installation. When installing polybutylene pipe with compression fittings, use a pipe stiffener to ensure the pipe maintains its shape and prevents it from collapsing under the pressure of the fitting. For optimal compression and a reliable seal, we recommend using copper olives instead of brass. Copper is a softer metal, which allows for better compression and a more secure fit.

## DOWNLOADS & FURTHER INFORMATION

DOWNLOAD DATA SHEET

DOWNLOAD BIM INFORMATION

INSTALLATION INSTRUCTIONS

DATA SHEETS